Current GBE Issues resolved here.

* Image is reduced ½ size in the FS direction
  + (DS Datwidth error) DS Dat Width =16 is sent
  + Resolved in the .XDLL
* Error 47 causes imaging to stop
  + Jobs will image but won’t release from the rip and bounce back to active queue
  + Resolved with .XDLL which closes the communication socket faster as the solution
* Corruption of the image. Happens on older CTPS eg 4300, 8300 with retrofit
  + Current resolution is change the xitron33.ini file
    - Strobe Speed = 125 rather than the 62.5
  + Will eventually be corrected in the plugin rather than the .ini file